The provisioning assigns an address range to the device, and adds it to the mesh network.
Complete the following steps in the nRF Mesh app:

1. Tap :guilabel:`Add node` to start scanning for unprovisioned mesh devices.
#. Select the |device name| device to connect to it.
#. Tap :guilabel:`Identify`, and then :guilabel:`Provision`, to provision the device.
#. When prompted, select an OOB method and follow the instructions in the app.

Once the provisioning is complete, the app returns to the Network screen.
