.. _bt_mesh_dtt_readme:

Generic Default Transition Time models
######################################

The Generic Default Transition Time (DTT) models are used to control the transition of any other states on any element.
The DTT Client can remotely control the default transition time state of the server.

The DTT models only use native types, and have no common model-specific types.


.. toctree::
   :maxdepth: 1
   :glob:
   :caption: Subpages:

   gen_dtt_srv.rst
   gen_dtt_cli.rst
