# Battery on HackberryPi_CM5

The battery used on HackberryPi_CM5 is Lipo battery with multiple certifications

```Dimension```: 83x50.5x10.1mm  
```Capacity```: 5000mah @ 3.7V, 18.5Wh  
```Battery Voltage```: 2.75-4.2V  
```Weight```: 84.4g  
```Connector```: PH2.0 2P  
```Battery overcurrent protection```: 5A

# Battery Foto
![image](https://github.com/user-attachments/assets/dd967207-a15c-49b6-8718-a3090722f99e)
