# Eniigma Keyboards ek60

* Keyboard Maintainer: [eniigmakeyboards](https://github.com/eniigmakeyboards) and [adamws](https://github.com/adamws)

Make example for this keyboard (after setting up your build environment):

    make eniigmakeyboards/ek60:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

Press and hold the reset button on the underside of the PCB while plugging in the cable to reset the bootloader.
