# nt750

A drop-in replacement PCB for the Leopold FC750R.

* Keyboard Maintainer: [Evyd13](https://github.com/Evyd13)
* Hardware Supported: nt750 PCB
* Hardware Availability: [GitHub](https://github.com/evyd13/nt-series/tree/main/nt-750)

## Flashing

In place of the DIP switches there is a small button. Press that to jump to the bootloader. 


Make example for this keyboard (after setting up your build environment):

    make evyd13/nt750:default

Flashing example for this keyboard:

    make evyd13/nt750:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
