# DirectPins

![Raspberry Pi Pico pinout guide](https://learn.adafruit.com/getting-started-with-raspberry-pi-pico-circuitpython/pinouts)

Easily assign keys to pins for your custom project using QMK Configurator.

* Keyboard Maintainer: [Jeff Epler](https://github.com/jepler)
* Hardware Supported: Raspberry Pi Pico, other RP2040 boards
* Hardware Availability: Raspberry Pi, SparkFun, Adafruit, other makers

Make example for this keyboard (after setting up your build environment):

    qmk compile -kb ez_maker/directpins/rp2040 -km default

Flashing example for this keyboard:

    qmk flash -kb ez_maker/directpins/rp2040 -km default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
