# ATLANTIS AK81_VE

![ATLANTIS AK81_VE](https://i.imgur.com/nfuocgS.jpeg)

A 75% hotswap keyboard with per key RGB backlighting, RGB underglow and a rotary encoder.

* Keyboard Maintainer: [fOmey](https://github.com/fOmey)
* Hardware Supported: AK75X@AK81_VE
* Hardware Availability: [AliExpress.com](https://aliexpress.com), [Shopee](https://shopee.com.my)

Make example for this keyboard (after setting up your build environment):

    make atlantis/ak81_ve:default

## Bootloader

Enter the bootloader in 2 ways:

* **Bootmagic reset**: Hold down the key at (0,0) in the matrix
* **Keycode in layout**: Press the key mapped to `QK_BOOT` if it is available
* **Physical reset pins**: Briefly short the reset pins using tweezers, a paperclip, or any other conductive material.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).