# Bloomer

![Bloomer](http://assets.cozykeys.xyz/images/keyboards/bloomer/bloomer-angle-2_800x800.jpg)

- Keyboard Maintainer: [Paul Ewing](https://github.com/pcewing)
- Hardware Supported: ItsyBitsy 32u4 5V 16MHz
- Hardware Availability: [Bloomer Repository](https://github.com/cozykeys/bloomer)

Make example for this keyboard (after setting up your build environment):

    make cozykeys/bloomer/v2:default  # for Bloomer v2
    make cozykeys/bloomer/v3:default  # for Bloomer v3

Flashing example for this keyboard:

    make cozykeys/bloomer/v2:default:flash  # for Bloomer v2
    make cozykeys/bloomer/v3:default:flash  # for Bloomer v3

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Flashing the Firmware

See the QMK docs for handwiring a keyboard; there is a section with instructions on how to flash the *.hex* file to the Teensy 2.0 controller.
