# Frooastboard Nano

![Frooastboard Nano](https://i.imgur.com/f26O8JLh.jpg)

* Keyboard Maintainer: [Frooastside](https://github.com/frooastside)
* Hardware Supported: Frooastboard Nano
* Hardware Availability: https://github.com/Frooastside/Frooastboard

**Reset Key:** Hold down the key located at `K00`, commonly programmed as ESCAPE while plugging in the keyboard. (If via is used it is the key located at `K10`.)

Make example for this keyboard (after setting up your build environment):

    make frooastboard/nano:default

Flashing example for this keyboard:

    make frooastboard/nano:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
