# SPRH

![SPRH](https://i.imgur.com/fkI5ryph.jpg)

SPRH (Square Peg-Round Hole) is a 65% ortholinear board compatibile with standard keycap sets.

* Keyboard Maintainer: [Eye Oh Designs](https://github.com/joedinkle)
* Hardware Supported: SPRH ver 1.00
* Hardware Availability: Groupbuy ran in April 2021

Make example for this keyboard (after setting up your build environment):

    make eyeohdesigns/sprh:default

Flashing example for this keyboard:

    make eyeohdesigns/sprh:default:flash

To enter the bootloader, either depress the reset button on the back of the PCB, or use the `QK_BOOT` keycode found on the function layer.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
