# Split65

An split 65% keyboard with two OLEDs

* Keyboard Maintainer: [Percy-JW2](https://github.com/PercyJW-2)
* Hardware Supported: ProMicro and compatibles, Proton C
* Hardware Availability: [Repository](https://github.com/PercyJW-2/Split65)

Make example for this keyboard with an ProMicro:

    make handwired/split65/promicro:default
    
Make example for this keyboard with an Proton C:

    make handwired/split65/stm32:default
    
Example for flashing this keyboard with an ProMicro

    make handwired/split65/promicro:default:flash

Example for flashing this keyboard with an Proton C

    make handwired/split65/stm32:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
