# Mercury65

![Mercury65](https://i.imgur.com/rjfARj3h.jpeg)

*65% Form Factor with a Separated Arrow Cluster used for Mercury65*


* Keyboard Maintainer: [Drewkeys](https://github.com/drewpyun)
* Hardware Supported: Made specifically for Mercury65, 65% hotswap supported
* Hardware Availability: https://www.rocketkeyboards.com/collections/mercury65/products/gb-mercury65-keyboard

Make example for this keyboard (after setting up your build environment):

    make drewkeys/mercury65:default

Flashing example for this keyboard:

    make drewkeys/mercury65:default:flash
## Bootloader

Resetting Board: Press the button on the PCB next to the spacebar to soft reset the board to reflash (bootloader mode).

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
