# Crazy Keyboard 68

![Front View of Crazy Keyboard 68 PCB](https://i.imgur.com/0nTjDbU.jpg)\
![Back View of Crazy Keyboard 68 PCB](https://i.imgur.com/gTpdux3.jpeg)

Obscure 68% hotswap PCB sold on taobao, powered by ATM32U4. RGB key lighting and underglow requires self-soldering.

* Keyboard Maintainer: [chent7](https://github.com/chent7)
* Hardware Supported: crazy keyboard 68 Standard
* Hardware Availability: [taobao.com](https://item.taobao.com/item.htm?spm=a1z09.2.0.0.19422e8dJUzj8d&id=605218560507)

Make example for this keyboard (after setting up your build environment):

    make crazy_keyboard_68:default

Flashing example for this keyboard:

    make crazy_keyboard_68:default:flash

## Layouts 

### ANSI
![Default ANSI Layout](https://i.imgur.com/y1ZApvU.png)

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
