# tenpad macropad

A 28 button macropad, in a format that is closest to a 5x6 grid, designed by evan cook
[Default Layout](https://raw.githubusercontent.com/evanmcook/sleepingdinosaur/main/images/layouts/sleepingdinosaurdefault.jpg)

* Keyboard Maintainer: [evan cook](https://github.com/evanmcook/)
* Hardware Supported: sleepingdinosaur Macropad PCB
* Hardware Availability: [tenpad Github](https://github.com/evanmcook/sleepingdinosaur)

Make example for this keyboard (after setting up your build environment):

    make evancookaudio/sleepingdinosaur:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Enter the bootloader: 
* **Physical reset button**: On the underside of the board, near the USB connector and microcontroller, press and hold the small button labeled reset for more than one second to enter the bootloader.