# Friedrich

![friedrich](https://i.imgur.com/LH15u37l.jpg)

A small printer friendly 3D printed 50% keyboard.

* Keyboard Maintainer: [kb-elmo](https://github.com/kb-elmo)
* Hardware Supported: Friedrich PCB by kb-elmo
* Hardware Availability: [Open source project](https://github.com/MarvFPV/Friedrich)

Make example for this keyboard (after setting up your build environment):

    make friedrich:default

Flashing example for this keyboard:

    make friedrich:default:flash

**Bootloader:** Press the physical reset button on the top side of the PCB or hold down ESC while plugging in the board.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
