# Lulu

![boardsource Lulu](https://i.imgur.com/tjvUoXTh.png)

The lulu is what the ergo community has needed for a long time, a high-end aesthetic split ergo 60%. With this project we not only tried to create a beautiful product but we also wanted to unify the some what split 60% community. With hotswap, per key rgb & underglow, swappable encoder and adjustable tenting with out giving up anything.


* Keyboard Maintainer: [Boardsource](https://github.com/daysgobye) 
* Hardware Supported: lulu v1
* Hardware Availability: this keyboard is available from the [Boardsource store](https://boardsource.xyz/store/61d0b772319a1f3cc53ba2fb)


Make example for this keyboard (after setting up your build environment):

    make boardsource/lulu/rp2040:default
    make boardsource/lulu/avr:default

Flashing example for this keyboard:

    make boardsource/lulu/rp2040:default:flash
    make boardsource/lulu/avr:default:flash


Compile `rp2040` firmware if you purchased PCB in lulu group buy (integrated microcontroller).
Compile `avr` firmware if your PCB uses a drop-in microcontroller like Pro Micro.


Enter bootloader by holding down the upper outer key while you plug in the usb cable, or by pushing the reset switch on the pcb.


See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
