# frankie_macropad

![frankie_macropad](https://i.imgur.com/X46CSH7h.jpg)

A simple 8-key macropad with two rotary encoders.

* Keyboard Maintainer: [Eric Wood](https://github.com/eric-wood)
* Hardware Supported: atmega16u2
* Hardware Availability: https://github.com/eric-wood/macro-pad

Make example for this keyboard (after setting up your build environment):

    make handwired/frankie_macropad:default

To switch to bootloader mode, unplug the keyboard and plug it back in while holding down the bottom left key.

Flashing example for this keyboard:

    make handwired/frankie_macropad:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
