# DirectPins

![Promicro Pinout Guide](https://i.imgur.com/LZ194Hf.jpg)

Easily assign keys to pins for your custom project using QMK Configurator.

* Keyboard Maintainer: [Zach White](https://github.com/skullydazed)
* Hardware Supported: Promicro
* Hardware Availability: Sparkfun, chinese clones

Make example for this keyboard (after setting up your build environment):

    qmk compile -kb ez_maker/directpins/promicro -km default

Flashing example for this keyboard:

    qmk flash -kb ez_maker/directpins/promicro -km default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
