# babyV

![babyV](https://i.imgur.com/iRUm9I5l.jpg)

babyV is a 40% ortholinear take on the EM7/Alice layout.

* Keyboard Maintainer: [Eye Oh Designs](https://github.com/joedinkle)
* Hardware Supported: babyV ver 1.00
* Hardware Availability: Groupbuy ran from Nov - Dec 2020

Make example for this keyboard (after setting up your build environment):

    make eyeohdesigns/babyv:default

Flashing example for this keyboard:

    make eyeohdesigns/babyv:default:flash
   
To enter the bootloader, either depress the reset button on the back of the PCB, or use the `QK_BOOT` keycode found on the function layer.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
