// Tabulated flux-factor for axi-symmetrical problems (more precisely, factor for heat-transfer coefficient variation).
// The distance (d, in m) is computed from the center of axi-symmetry (defined in file /constant/setCase).

// d (m)	flux factor	pressure factor
0.000e-2	1.000		1
1.000e-2	0.8		1
2.000e-2	0.2		1
3.000e-2	0.05		1
10.000e-2	0.0		1

